Review of Asbestos Management Plan – April 2017

4 Phases: Identification, Evaluation, Control and Monitoring

* Anyone conducting work that may result in disturbance to ACM must check the onsite register.
* A permit to work system must be engaged for any works that may result in disturbance to ACM.
* Any work undertaken that may disturb ACM must be performed in such a way that either avoids exposure or is performed with appropriate and effective controls in place to minimise disturbance and exposure to persons.
* Only suitable contractors or consultants may carry out asbestos related work and only licensed contractors may remove asbestos.
* DOE Hygienist to be used arranging for inspections, risk assess etc. of asbestos.
* No free landfill from construction sites allowed. Must obtain from reputable supplier with certificate if required.